P-filament 721

*Product:* [*https://www.ppprint.de/en/produkt/p-filament-721-white/#:~:text=Printed%20parts%20of%20'P%2Dfilament,excellently%20suited%20for%20lightweight%20construction*](https://www.ppprint.de/en/produkt/p-filament-721-white/#:~:text=Printed%20parts%20of%20'P%2Dfilament,excellently%20suited%20for%20lightweight%20construction)

**Datasheet:** <https://www.ppprint.de/wp-content/uploads/2021/01/P-filament-721-Datenblatt-deutsch.pdf>

* **Density:** 0.9 [g/cm^3]

A white background with black dots

Description automatically generated

* **E-Modul:** 640 ± 20, 660 ± 10 [MPa]
* **Yield Strength:** 18.1 ± 0.1, 19.6 ± 0.3 [MPa]
* **Tensile Strength:** 18.7 ± 0.3, 35.1 ± 0.6 [MPa]
* **Elongation:** >600

**ISO-1133:**